,Maximum Air Flow##HVAC_AIR_FLOW##CUBIC_FEET_PER_MINUTE,Maximum Static Pressure##HVAC_PRESSURE##INCHES_OF_WATER,Fan Speed (RPM)##OTHER##,Shipping Weight (lbs)##OTHER##,Overall Width(A)##LENGTH##INCHES,Venturi Orifice Opening(B Dia)##LENGTH##INCHES,Fan Inside Depth(D max)##LENGTH##INCHES,Panel Depth(E)##LENGTH##INCHES,Venturi Depth(F)##LENGTH##INCHES
BCH24,0,0,0,0,28,25,16,3,3
BCH30,0,0,0,0,34,31,18,2.5,3
BCH36,0,0,0,0,40,37,20,3,4.75
BCH42,0,0,0,0,46,43,22,3.75,4.5
BCH48,0,0,0,0,54,49,25,2.75,4.75
BCH54,0,0,0,0,60,55,28,3,5
BCH60,0,0,0,0,66,61,28,2.75,6
